Milestone One

Zachary Derepentigny

What does pwmled2 set the PWM period to?

**Pwmled2 sets the PWM period to 3000 milliseconds.**

Which PWM\_xxx() function sets the PWM period?

**PWM\_setPeriod sets the PWM period of a specified handle.**

Which PWM\_xxx() function sets the PWM duty cycle?

**PWM\_setDuty sets the duty cycle of a specified handle.**

What is the purpose of the while(1) loop in pwmled2?

**The while loop is used to set an infinite loop so that pwmled2 keeps running.**

What is the purpose of usleep() in the while(1) loop?

**Usleep creates a pause in the execution of pwmled2 which allows it to produce the blinking effect we are trying to implement.**